========================================================================
		Setup for Cross Chip Trunk
========================================================================

This sample shows how to setup the Cross Chip Trunk with the following 
assumptions.
	Assumption 1: Device ID, Cascading Port, CPU Port, and Interswitch Port are
		already set properly. For more information, please refer to the 
		sample/MultiDevice/msApiInit.c

	Assumption 2: Port 0,1,2 of Device 0 and Port 0 of Device 1 are member of a 
		trunk with Trunk ID, 1.







