HOSTAPD(8)

NAME
hostapd - IEEE 802.11 AP, IEEE 802.1X/WPA/WPA2/EAP/RADIUS Authenticator

SYNOPSIS
hostapd [-hdBKtv] [-P <PID file>] <configuration file(s)>

DESCRIPTION
This manual page documents briefly the hostapd daemon.

hostapd is a user space daemon for access point and authentication servers. It implements IEEE 802.11 access point management, IEEE 802.1X/WPA/WPA2/EAP Authenticators and RADIUS authentication server. The current version supports Linux (Host AP, madwifi, mac80211-based drivers) and FreeBSD (net80211). hostapd is designed to be a "daemon" program that runs in the background and acts as the backend component controlling authentication. hostapd supports separate frontend programs and an example text-based frontend, hostapd_cli, is included with hostapd.

OPTIONS
A summary of options is included below. For a complete description, run hostapd from the command line.

-h  Show usage.

-d  Show more debug messages.

-dd Show even more debug messages.

-B  Run daemon in the background.

-P <PID file>
    Path to PID file.

-K  Include key data in debug messages.

-t  Include timestamps in some debug messages.

-v  Show hostapd version.

SEE ALSO
hostapd_cli(1).

AUTHOR
hostapd was written by Jouni Malinen <j@w1.fi>.

This manual page was written by Faidon Liambotis <faidon@cube.gr>, for the Debian project (but may be used by others).