HOSTAPD_CLI(1)

NAME
hostapd_cli - hostapd command-line interface

SYNOPSIS
hostapd_cli [-p<path>] [-i<ifname>] [-a<path>] [-hvB] [command..]

DESCRIPTION
This manual page documents briefly the hostapd_cli utility.

hostapd_cli is a command-line interface for the hostapd daemon. hostapd is a user space daemon for access point and authentication servers. It implements IEEE 802.11 access point management, IEEE 802.1X/WPA/WPA2/EAP Authenticators and RADIUS authentication server. For more information about hostapd refer to the hostapd(8) man page.

OPTIONS
A summary of options is included below. For a complete description, run hostapd_cli from the command line.

-p<path>
    Path to find control sockets. Default: /var/run/hostapd

-i<ifname>
    Interface to listen on. Default: first interface found in socket path.

-a<path>
    Run in daemon mode executing the action file based on events from hostapd.

-B  Run a daemon in the background.

-h  Show usage.

-v  Show hostapd_cli version.

COMMANDS
A summary of commands is included below. For a complete description, run hostapd_cli from the command line.

mib Get MIB variables (dot1x, dot11, radius).

sta <addr>
    Get MIB variables for one station.

all_sta
    Get MIB variables for all stations.

help
    Get usage help.

interface [ifname]
    Show interfaces/select interface.

level <debug level>
    Change debug level.

license
    Show full hostapd_cli license.

quit
    Exit hostapd_cli.

SEE ALSO
hostapd(8).

AUTHOR
hostapd_cli was written by Jouni Malinen <j@w1.fi>.

This manual page was written by Faidon Liambotis <faidon@cube.gr>, for the Debian project (but may be used by others).